Input #0, mpegts, from '/home/mfritsche/fourier-test/bbb_720p10s_mpeg2.ts':
  Duration: 00:00:10.00, start: 1.441667, bitrate: 4202 kb/s
  Program 1 
    Metadata:
      service_name    : Service01
      service_provider: FFmpeg
  Stream #0:0[0x100]: Video: mpeg2video (Main) ([2][0][0][0] / 0x0002), yuv420p(tv, bt709, progressive), 1280x720 [SAR 1:1 DAR 16:9], 24 fps, 24 tbr, 90k tbn, start 1.441667
    Side data:
      CPB properties: bitrate max/min/avg: 0/0/0 buffer size: 1130496 vbv_delay: N/A
Stream mapping:
  Stream #0:0 -> #0:0 (mpeg2video (native) -> wrapped_avframe (native))
Press [q] to stop, [?] for help
v4l2-request: cap_pool_init: 24 slots ready (v4l2_index=0..23, 1 plane(s) per slot)
v4l2-request: Unable to set control(s): Invalid argument
Output #0, null, to 'pipe:':
  Metadata:
    encoder         : Lavf62.12.100
  Stream #0:0: Video: wrapped_avframe, nv12(tv, bt709, progressive), 1280x720 [SAR 1:1 DAR 16:9], q=2-31, 200 kb/s, 24 fps, 24 tbn
    Metadata:
      encoder         : Lavc62.28.100 wrapped_avframe
[out#0/null @ 0xaaaabf90c500] video:2KiB audio:0KiB subtitle:0KiB other streams:0KiB global headers:0KiB muxing overhead: unknown
frame=    5 fps=0.0 q=-0.0 Lsize=N/A time=00:00:00.20 bitrate=N/A speed=1.46x elapsed=0:00:00.14    
